conf3

Seite 1 fadc 113- 246 an 12 b13 an 11 b12 an 10 b11 an 9 b10 an 8 b9 an 7 b8 an 6 b7 an 5 b6 an 4 b5 an 3 b4 an 2 b3 an 1 b2

tdc configuration

word tdc1 tdc2 tdc3 tdc4 tdc5 tdc6 tdc7 tdc8 tdc9 tdc10 4 TPC A TPC B TPC C TPC D PC 1A PC 6A PC 3A PC 3C an low an low an low an low 3 TPC A TPC B TPC C TPC D PC 1B PC 6B PC 3B PC3 D an high an high an high an high 2 s1,s2,s2a TPC A TPC B TPC A TPC B PC 2 syc bits pulser e1,e2 strip low strip low strip high strip high 1 clock clock clock clock clock clock clock clock clock clock

pulser tdc9/b8 and tdc1/b5 used as pulser tag bit pulse 100mV DAC gives 40 mV @ disciminator

Tom describe additional overflow bit

20

PC4B 9- 24

PC4A 1- 8 PC5A 1- 8 PC5B 9- 24